{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["义龙新区龙广镇康雅庭小区建设工程未完工程一览表"]
["序号","项目名称","单位","工程量","单价","合价","备注"]
["一","室外附属工程"]
[1,"道路(车行道)级配碎石垫层25cm厚","m²",4100]
[2,"道路水泥稳定层（水泥含量6%）20cm厚","m²",4100]
[3,"道路沥青混凝土路面（中粒式）5cm厚","m²",4100]
[4,"道路沥青混凝土路面（细粒式）3cm厚","m²",4100]
[5,"青石路缘石（规格60cm×50cm×10cm)","m",1050]
[6,"人行横道10cm厚碎石垫层","m²",1800]
[7,"人行横道10cm厚C20混凝土垫层","m²",1800]
[8,"人行横道青石板铺贴","m²",1800]
[9,"桂花树（四季桂 胸径15cm）","株",30]
[10,"桂花树（八月桂 胸径15cm）","株",30]
[11,"马尼拉草坪","m²",650]
[12,"停车位级配碎石垫层10cm厚","m²",2000]
[13,"停车位水泥稳定层（水泥含量6%）20cm厚","m²",2000]
[14,"停车位沥青混凝土路面（细粒式）4cm厚","m²",2000]
[15,"室外小广场10cm厚碎石垫层","m²",600]
[16,"室外小广场青石板铺贴","m²",600]
["二","房屋建筑工程"]
[1,"金属窗 铝合金推拉窗(成品)安装（中空玻璃5+16A+5）","m²",270]
[2,"飘窗 铝合金推拉窗(成品)安装（中空玻璃5+16A+5）","m²",830]
[3,"中空玻璃（中空玻璃5+16A+5）","m²",1700,null,null,"窗框已装"]